# Enabling second output

xrandr --output VGA_1 --auto | xrandr --output DVI-D_1 --auto
--- | ---
(II) RADEONHD(0): FUNCTION: rhdRRXF86CrtcResize (II) RADEONHD(0): FUNCTION: rhdRROutputModeFixup | (II) RADEONHD(0): FUNCTION: rhdRRXF86CrtcResize (II) RADEONHD(0): FUNCTION: rhdRROutputModeFixup
(II) RADEONHD(0): FUNCTION: DigAllocFree (II) RADEONHD(0): rhdRRFreeOutputs: Freeing Output: UNIPHY_A (II) RADEONHD(0): rhdRROutputModeFixup: Output VGA_1 : n/a | (II) RADEONHD(0): rhdRROutputModeFixup: Output DVI-D_1 : n/a (II) RADEONHD(0): FUNCTION: DigAllocFree (II) RADEONHD(0): Mapping DIG1 encoder to UNIPHYA
(II) RADEONHD(0): FUNCTION: RHDRRModeFixup (II) RADEONHD(0): FUNCTION: DxFBValid: CRTC 2 (II) RADEONHD(0): DxModeValid: CRTC 2 | (II) RADEONHD(0): FUNCTION: RHDRRModeFixup (II) RADEONHD(0): FUNCTION: DxFBValid: CRTC 2 (II) RADEONHD(0): DxModeValid: CRTC 2
(II) RADEONHD(0): FUNCTION: DACModeValid | (II) RADEONHD(0): FUNCTION: DigModeValid (II) RADEONHD(0): FUNCTION: ATOMTransmitterModeValid (II) RADEONHD(0): FUNCTION: EncoderModeValid
(II) RADEONHD(0): FUNCTION: rhdRROutputPrepare (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdBIOSScratchSetDeviceForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState | (II) RADEONHD(0): FUNCTION: rhdRROutputPrepare (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdBIOSScratchSetDeviceForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState
(II) RADEONHD(0): FUNCTION: DACAPowerRV620 | (II) RADEONHD(0): DigPower(UNIPHY_A,POWER_RESET) (II) RADEONHD(0): FUNCTION: ATOMTransmitterPower (II) RADEONHD(0): ATOMTransmitterPower: DIGn_CNTL: n=1: 0x0 n=2: 0x110 (II) RADEONHD(0): FUNCTION: rhdAtomDigTransmitterControl (II) RADEONHD(0): Calling UNIPHYTransmitterControl (II) RADEONHD(0): Pspace[01]: 0x08000000 (II) RADEONHD(0): Pspace[02]: 0x00000000 (II) RADEONHD(0): FUNCTION: RHDAtomBiosFunc (II) RADEONHD(0): FUNCTION: rhdAtomExec (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): ParseTable said: CD_SUCCESS (II) RADEONHD(0): Call to AtomBIOS Exec succeeded (II) RADEONHD(0): UNIPHYTransmitterControl Successful (II) RADEONHD(0): ATOMTransmitterPower: DIGn_CNTL: n=1: 0x0 n=2: 0x110 (II) RADEONHD(0): FUNCTION: EncoderPower (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x0 n=2: 0x110 (II) RADEONHD(0): EncoderPower(RHD_POWER_SHUTDOWN, 1) (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x0 n=2: 0x110
(II) RADEONHD(0): FUNCTION: rhdRRCrtcPrepare (II) RADEONHD(0): FUNCTION: D2Power (II) RADEONHD(0): rhdRRCrtcModeSet: CRTC 2 : n/a at 0/0 (II) RADEONHD(0): On Crtc 1 Setting 60.0 Hz Mode: Modeline "n/a" 122.00 1400 1488 1640 1880 1050 1052 1064 1082 +hsync +vsync (II) RADEONHD(0): FUNCTION: DxFBSet: CRTC 2 (2560[2560]x2560@24bpp) +0x8000 ) (II) RADEONHD(0): FUNCTION: DxModeSet: CRTC 2 (II) RADEONHD(0): DxModeSet: Setting Modeline "n/a" 122.00 1400 1488 1640 1880 1050 1052 1064 1082 +hsync +vsync (II) RADEONHD(0): FUNCTION: DxScaleSet: CRTC 2 viewport: 1400x1050 (II) RADEONHD(0): FUNCTION: DxScaleSet: CRTC 2 viewport: 1400x1050 - OverScan: T: 0 B: 0 R: 0 L: 0 None (II) RADEONHD(0): FUNCTION: RHDMCTuneAccessForDisplay (II) RADEONHD(0): FUNCTION: D2ViewPortStart (II) RADEONHD(0): RHDPLLSet: Setting PLL 2 to 122000kHz (II) RADEONHD(0): PLL Calculation: 122000kHz = (((27000 / 0x9) * 0xF4) / 0x6) (0kHz off) (II) RADEONHD(0): FUNCTION: RV620DCCGCLKAvailable (II) RADEONHD(0): FUNCTION: RV620PLL2Set (II) RADEONHD(0): FUNCTION: RV620PLL2SetLow (II) RADEONHD(0): FUNCTION: PLL2Calibrate (II) RADEONHD(0): PLL2Calibrate: lock in 148 loops (II) RADEONHD(0): FUNCTION: D2LUTSelect (II) RADEONHD(0): RHDLUTCopyForRR: LUT B (II) RADEONHD(0): FUNCTION: rhdRROutputModeSet (II) RADEONHD(0): rhdRROutputModeSet: Output VGA_1 : n/a to CRTC 2 (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdBIOSScratchSetDeviceForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchSetCrtcState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState | (II) RADEONHD(0): FUNCTION: rhdRRCrtcPrepare (II) RADEONHD(0): FUNCTION: D2Power (II) RADEONHD(0): rhdRRCrtcModeSet: CRTC 2 : n/a at 0/0 (II) RADEONHD(0): On Crtc 1 Setting 60.0 Hz Mode: Modeline "n/a" 148.50 1920 2008 2052 2200 1080 1084 1089 1125 +hsync +vsync (II) RADEONHD(0): FUNCTION: DxFBSet: CRTC 2 (2560[2560]x2560@24bpp) +0x8000 ) (II) RADEONHD(0): FUNCTION: DxModeSet: CRTC 2 (II) RADEONHD(0): DxModeSet: Setting Modeline "n/a" 148.50 1920 2008 2052 2200 1080 1084 1089 1125 +hsync +vsync (II) RADEONHD(0): FUNCTION: DxScaleSet: CRTC 2 viewport: 1920x1080 (II) RADEONHD(0): FUNCTION: DxScaleSet: CRTC 2 viewport: 1920x1080 - OverScan: T: 0 B: 0 R: 0 L: 0 None (II) RADEONHD(0): FUNCTION: RHDMCTuneAccessForDisplay (II) RADEONHD(0): FUNCTION: D2ViewPortStart (II) RADEONHD(0): RHDPLLSet: Setting PLL 2 to 148500kHz (II) RADEONHD(0): PLL Calculation: 148500kHz = (((27000 / 0x2) * 0x37) / 0x5) (0kHz off) (II) RADEONHD(0): FUNCTION: RV620DCCGCLKAvailable (II) RADEONHD(0): FUNCTION: RV620PLL2Set (II) RADEONHD(0): FUNCTION: RV620PLL2SetLow (II) RADEONHD(0): FUNCTION: PLL2Calibrate (II) RADEONHD(0): PLL2Calibrate: lock in 46 loops (II) RADEONHD(0): FUNCTION: D2LUTSelect (II) RADEONHD(0): RHDLUTCopyForRR: LUT B (II) RADEONHD(0): FUNCTION: rhdRROutputModeSet (II) RADEONHD(0): rhdRROutputModeSet: Output DVI-D_1 : n/a to CRTC 2 (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdBIOSScratchSetDeviceForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchSetCrtcState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState
(II) RADEONHD(0): FUNCTION: DACASetRV620 (II) RADEONHD(0): FUNCTION: RHDAtomBiosFunc (II) RADEONHD(0): FUNCTION: rhdAtomCompassionateDataQuery (**) RADEONHD(0): Call to DAC1 BG Adjustment failed (II) RADEONHD(0): FUNCTION: RHDAtomBiosFunc (II) RADEONHD(0): FUNCTION: rhdAtomCompassionateDataQuery (**) RADEONHD(0): Call to DAC1 DAC Adjustment failed (II) RADEONHD(0): FUNCTION: RHDAtomBiosFunc (II) RADEONHD(0): FUNCTION: rhdAtomGetDataInCodeTable (II) RADEONHD(0): Call to AtomBIOS Get Datatable from Codetable succeeded (II) RADEONHD(0): DACGetElectrical: WhiteFine found in Code Table. (II) RADEONHD(0): DACGetElectrical: DAC[0] BandGap: 0x00 WhiteFine: 0x20 | (II) RADEONHD(0): FUNCTION: DigMode (II) RADEONHD(0): FUNCTION: EncoderSet (II) RADEONHD(0): EncoderSet: DIGn_CNTL: n=1: 0x0 n=2: 0x110 (II) RADEONHD(0): FUNCTION: TMDSEncoder
(II) RADEONHD(0): FUNCTION: DxFMTSet | (II) RADEONHD(0): FUNCTION: DxFMTSet (II) RADEONHD(0): EncoderSet: DIGn_CNTL: n=1: 0x301 n=2: 0x110 (II) RADEONHD(0): FUNCTION: ATOMTransmitterSet (II) RADEONHD(0): ATOMTransmitterSet: DIGn_CNTL: n=1: 0x301 n=2: 0x110 (II) RADEONHD(0): FUNCTION: rhdAtomDigTransmitterControl (II) RADEONHD(0): Calling UNIPHYTransmitterControl (II) RADEONHD(0): Pspace[01]: 0x0a00e808 (II) RADEONHD(0): Pspace[02]: 0x00000000 (II) RADEONHD(0): FUNCTION: RHDAtomBiosFunc (II) RADEONHD(0): FUNCTION: rhdAtomExec (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): ParseTable said: CD_SUCCESS (II) RADEONHD(0): Call to AtomBIOS Exec succeeded (II) RADEONHD(0): UNIPHYTransmitterControl Successful (II) RADEONHD(0): ATOMTransmitterSet: DIGn_CNTL: n=1: 0x301 n=2: 0x110 (II) RADEONHD(0): FUNCTION: RHDHdmiSetMode (II) RADEONHD(0): FUNCTION: RHDAudioSetClock (II) RADEONHD(0): RHDAudioSetClock: using UNIPHY_A as clock source with 148500 khz (II) RADEONHD(0): Using ACR timing N=4096 CTS=148500 for frequency 32000 (II) RADEONHD(0): Using ACR timing N=6272 CTS=165000 for frequency 44100 (II) RADEONHD(0): Using ACR timing N=6144 CTS=148500 for frequency 48000
(II) RADEONHD(0): FUNCTION: rhdRRCrtcCommit (II) RADEONHD(0): FUNCTION: D2Power (II) RADEONHD(0): State at CRTC 2: RRCrtc #0 [rhd CRTC 1]: active 1 [1] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1400x1050) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc CRTC 2 [CRTC 2] [inactive] connected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc CRTC 1 [CRTC 1] [active] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc null [null] [inactive] disconnected (II) RADEONHD(0): FUNCTION: rhdRROutputCommit (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdBIOSScratchSetDeviceForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchSetCrtcState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState | (II) RADEONHD(0): FUNCTION: rhdRRCrtcCommit (II) RADEONHD(0): FUNCTION: D2Power (II) RADEONHD(0): State at CRTC 2: RRCrtc #0 [rhd CRTC 1]: active 1 [1] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1920x1080) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc null [null] [inactive] disconnected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc CRTC 1 [CRTC 1] [active] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc CRTC 2 [CRTC 2] [inactive] connected (II) RADEONHD(0): FUNCTION: rhdRROutputCommit (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdBIOSScratchSetDeviceForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchSetCrtcState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState
(II) RADEONHD(0): FUNCTION: DACAPowerRV620 (II) RADEONHD(0): State at VGA_1: RRCrtc #0 [rhd CRTC 1]: active 1 [1] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1400x1050) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc CRTC 2 [CRTC 2] [active] connected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc CRTC 1 [CRTC 1] [active] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc null [null] [inactive] disconnected (II) RADEONHD(0): rhdRROutputDpms: Output DVI-D_1 : Off (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState (II) RADEONHD(0): DigPower(UNIPHY_A,POWER_SHUTDOWN) | (II) RADEONHD(0): DigPower(UNIPHY_A,POWER_ON) (II) RADEONHD(0): FUNCTION: EncoderPower (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x301 n=2: 0x110 (II) RADEONHD(0): EncoderPower(RHD_POWER_ON, 1) (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x311 n=2: 0x110
(II) RADEONHD(0): FUNCTION: ATOMTransmitterPower (II) RADEONHD(0): ATOMTransmitterPower: DIGn_CNTL: n=1: 0x0 n=2: 0x110 (II) RADEONHD(0): FUNCTION: rhdAtomDigTransmitterControl (II) RADEONHD(0): Calling UNIPHYTransmitterControl (II) RADEONHD(0): Pspace[01]: 0x08000000 (II) RADEONHD(0): Pspace[02]: 0x00007f65 (II) RADEONHD(0): FUNCTION: RHDAtomBiosFunc (II) RADEONHD(0): FUNCTION: rhdAtomExec (II) RADEONHD(0): FUNCTION: atomSaveRegisters | (II) RADEONHD(0): FUNCTION: ATOMTransmitterPower (II) RADEONHD(0): ATOMTransmitterPower: DIGn_CNTL: n=1: 0x311 n=2: 0x110 (II) RADEONHD(0): FUNCTION: rhdAtomDigTransmitterControl (II) RADEONHD(0): Calling UNIPHYTransmitterControl (II) RADEONHD(0): Pspace[01]: 0x0100e808 (II) RADEONHD(0): Pspace[02]: 0x00000000 (II) RADEONHD(0): FUNCTION: RHDAtomBiosFunc (II) RADEONHD(0): FUNCTION: rhdAtomExec (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters
(II) RADEONHD(0): ParseTable said: CD_SUCCESS (II) RADEONHD(0): Call to AtomBIOS Exec succeeded (II) RADEONHD(0): UNIPHYTransmitterControl Successful (II) RADEONHD(0): FUNCTION: rhdAtomDigTransmitterControl (II) RADEONHD(0): Calling UNIPHYTransmitterControl (II) RADEONHD(0): Pspace[01]: 0x00000000 (II) RADEONHD(0): Pspace[02]: 0x00007f65 (II) RADEONHD(0): FUNCTION: RHDAtomBiosFunc (II) RADEONHD(0): FUNCTION: rhdAtomExec (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters | (II) RADEONHD(0): ParseTable said: CD_SUCCESS (II) RADEONHD(0): Call to AtomBIOS Exec succeeded (II) RADEONHD(0): UNIPHYTransmitterControl Successful (II) RADEONHD(0): FUNCTION: rhdAtomDigTransmitterControl (II) RADEONHD(0): Calling UNIPHYTransmitterControl (II) RADEONHD(0): Pspace[01]: 0x0900e808 (II) RADEONHD(0): Pspace[02]: 0x0002e808 (II) RADEONHD(0): FUNCTION: RHDAtomBiosFunc (II) RADEONHD(0): FUNCTION: rhdAtomExec (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters
(II) RADEONHD(0): ParseTable said: CD_SUCCESS (II) RADEONHD(0): Call to AtomBIOS Exec succeeded (II) RADEONHD(0): UNIPHYTransmitterControl Successful (II) RADEONHD(0): ATOMTransmitterPower: DIGn_CNTL: n=1: 0x0 n=2: 0x110 | (II) RADEONHD(0): ParseTable said: CD_SUCCESS (II) RADEONHD(0): Call to AtomBIOS Exec succeeded (II) RADEONHD(0): UNIPHYTransmitterControl Successful (II) RADEONHD(0): ATOMTransmitterPower: DIGn_CNTL: n=1: 0x311 n=2: 0x110
(II) RADEONHD(0): FUNCTION: EncoderPower (II) RADEONHD(0): digProbeEncoder: detected ENCODER_DIG1 for UNIPHYA (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x0 n=2: 0x110 (II) RADEONHD(0): EncoderPower(RHD_POWER_SHUTDOWN, 1) (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x0 n=2: 0x110 (II) RADEONHD(0): FUNCTION: RHDHdmiEnable | (II) RADEONHD(0): FUNCTION: RHDHdmiEnable (II) RADEONHD(0): State at DVI-D_1: RRCrtc #0 [rhd CRTC 1]: active 1 [1] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1920x1080) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc null [null] [inactive] disconnected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc CRTC 1 [CRTC 1] [active] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc CRTC 2 [CRTC 2] [active] connected (II) RADEONHD(0): rhdRROutputDpms: Output VGA_1 : Off (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState (II) RADEONHD(0): FUNCTION: DACAPowerRV620
(II) RADEONHD(0): State at POST-OutputDpms: RRCrtc #0 [rhd CRTC 1]: active 1 [1] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1400x1050) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc CRTC 2 [CRTC 2] [active] connected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc CRTC 1 [CRTC 1] [active] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc null [null] [inactive] disconnected | (II) RADEONHD(0): State at POST-OutputDpms: RRCrtc #0 [rhd CRTC 1]: active 1 [1] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1920x1080) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc null [null] [inactive] disconnected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc CRTC 1 [CRTC 1] [active] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc CRTC 2 [CRTC 2] [active] connected

# Disabling PANEL

xrandr --output PANEL --off
leaving VGA_1 | laeving DVI-D_1 (doesn't work)
--- | ---
(II) RADEONHD(0): rhdRROutputDpms: Output PANEL : Off (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdBIOSScratchSetDeviceForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchSetCrtcState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState (II) RADEONHD(0): DigPower(UNIPHY_KLDSKP_LVTMA,POWER_SHUTDOWN) (II) RADEONHD(0): FUNCTION: LVTMA_LVDSTransmitterPower (II) RADEONHD(0): FUNCTION: LVTMA_LVDSTransmitterPower (II) RADEONHD(0): FUNCTION: EncoderPower (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x0 n=2: 0x110 (II) RADEONHD(0): EncoderPower(RHD_POWER_SHUTDOWN, 2) (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x0 n=2: 0x100 | (II) RADEONHD(0): rhdRROutputDpms: Output VGA_1 : Off (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState (II) RADEONHD(0): FUNCTION: DACAPowerRV620
(II) RADEONHD(0): State at POST-OutputDpms: RRCrtc #0 [rhd CRTC 1]: active 0 [1] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1400x1050) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc CRTC 2 [CRTC 2] [active] connected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc null [CRTC 1] [inactive] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc null [null] [inactive] disconnected | (II) RADEONHD(0): State at POST-OutputDpms: RRCrtc #0 [rhd CRTC 1]: active 0 [1] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1920x1080) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc null [null] [inactive] disconnected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc null [CRTC 1] [active] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc CRTC 2 [CRTC 2] [active] connected
(II) RADEONHD(0): rhdRROutputDpms: Output DVI-D_1 : Off (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState (II) RADEONHD(0): DigPower(UNIPHY_A,POWER_SHUTDOWN) (II) RADEONHD(0): FUNCTION: ATOMTransmitterPower (II) RADEONHD(0): ATOMTransmitterPower: DIGn_CNTL: n=1: 0x0 n=2: 0x100 (II) RADEONHD(0): FUNCTION: rhdAtomDigTransmitterControl (II) RADEONHD(0): Calling UNIPHYTransmitterControl (II) RADEONHD(0): Pspace[01]: 0x08000000 (II) RADEONHD(0): Pspace[02]: 0x00007ffe (II) RADEONHD(0): FUNCTION: RHDAtomBiosFunc (II) RADEONHD(0): FUNCTION: rhdAtomExec (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): ParseTable said: CD_SUCCESS (II) RADEONHD(0): Call to AtomBIOS Exec succeeded (II) RADEONHD(0): UNIPHYTransmitterControl Successful (II) RADEONHD(0): FUNCTION: rhdAtomDigTransmitterControl (II) RADEONHD(0): Calling UNIPHYTransmitterControl (II) RADEONHD(0): Pspace[01]: 0x00000000 (II) RADEONHD(0): Pspace[02]: 0x00007ffe (II) RADEONHD(0): FUNCTION: RHDAtomBiosFunc (II) RADEONHD(0): FUNCTION: rhdAtomExec (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): FUNCTION: atomSaveRegisters (II) RADEONHD(0): ParseTable said: CD_SUCCESS (II) RADEONHD(0): Call to AtomBIOS Exec succeeded (II) RADEONHD(0): UNIPHYTransmitterControl Successful (II) RADEONHD(0): ATOMTransmitterPower: DIGn_CNTL: n=1: 0x0 n=2: 0x100 (II) RADEONHD(0): FUNCTION: EncoderPower (II) RADEONHD(0): digProbeEncoder: detected ENCODER_DIG1 for UNIPHYA (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x0 n=2: 0x100 (II) RADEONHD(0): EncoderPower(RHD_POWER_SHUTDOWN, 1) (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x0 n=2: 0x100 (II) RADEONHD(0): FUNCTION: RHDHdmiEnable | (II) RADEONHD(0): rhdRROutputDpms: Output PANEL : Off (II) RADEONHD(0): FUNCTION: rhdBIOSScratchUpdateBIOSScratchForOutput (II) RADEONHD(0): FUNCTION: rhdBIOSScratchSetDeviceForOutput (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchSetCrtcState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateOnState (II) RADEONHD(0): FUNCTION: rhdAtomBIOSScratchUpdateAttachedState (II) RADEONHD(0): DigPower(UNIPHY_KLDSKP_LVTMA,POWER_SHUTDOWN) (II) RADEONHD(0): FUNCTION: LVTMA_LVDSTransmitterPower (II) RADEONHD(0): FUNCTION: LVTMA_LVDSTransmitterPower (II) RADEONHD(0): FUNCTION: EncoderPower (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x211 n=2: 0x110 (II) RADEONHD(0): EncoderPower(RHD_POWER_SHUTDOWN, 2) (II) RADEONHD(0): EncoderPower: DIGn_CNTL: n=1: 0x211 n=2: 0x100
(II) RADEONHD(0): State at POST-OutputDpms: RRCrtc #0 [rhd CRTC 1]: active 0 [1] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1400x1050) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc CRTC 2 [CRTC 2] [active] connected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc null [CRTC 1] [inactive] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc null [null] [inactive] disconnected (II) RADEONHD(0): rhdRRCrtcDpms: CRTC 1: Off (II) RADEONHD(0): FUNCTION: D1Power (II) RADEONHD(0): D1CRTCDisable: 0 loops (II) RADEONHD(0): FUNCTION: RV620PLL1Power (II) RADEONHD(0): FUNCTION: RV620DCCGCLKSet | (II) RADEONHD(0): State at POST-OutputDpms: RRCrtc #0 [rhd CRTC 1]: active 0 [1] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1920x1080) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc null [null] [inactive] disconnected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc null [CRTC 1] [inactive] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc CRTC 2 [CRTC 2] [active] connected (II) RADEONHD(0): rhdRRCrtcDpms: CRTC 1: Off (II) RADEONHD(0): FUNCTION: D1Power (II) RADEONHD(0): D1CRTCDisable: 0 loops (II) RADEONHD(0): FUNCTION: RV620PLL1Power (II) RADEONHD(0): FUNCTION: RV620DCCGCLKSet
(II) RADEONHD(0): State at POST-CrtcDpms: RRCrtc #0 [rhd CRTC 1]: active 0 [0] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1400x1050) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc CRTC 2 [CRTC 2] [active] connected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc null [CRTC 1] [inactive] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc null [null] [inactive] disconnected (II) RADEONHD(0): FUNCTION: rhdRRXF86CrtcResize | (II) RADEONHD(0): State at POST-CrtcDpms: RRCrtc #0 [rhd CRTC 1]: active 0 [0] mode (1600x900) +0+0 RRCrtc #1 [rhd CRTC 2]: active 1 [1] mode unnamed (1920x1080) +0+0 RROut VGA_1 [Out DAC A Conn VGA 1] Crtc null [null] [inactive] disconnected RROut PANEL [Out UNIPHY_KLDSKP_LVTMA Conn PANEL] Crtc null [CRTC 1] [inactive] connected RROut DVI-D_1 [Out UNIPHY_A Conn DVI-D 1] Crtc CRTC 2 [CRTC 2] [active] connected