### System View
Use this page to get the summary on the existing configuration of your device.
Device | DSL
Model: | Viking | Operational Status: | Showtime/Data
H/W Version: | 81001a | Last State: | 0x0
S/W Version: | 21040407a2.3 | DSL Version: | Y218
Serial Number: | 123456789abcdx | Standard: | Multimode
Mode: | Routing | Up | Down
Up Time: | 42:23:12 | Speed | Latency | Speed | Latency
Time: | Mon Jan 05 23:14:25 1970 | 256 Kbps | Fast | 1024 Kbps | Fast
Time Zone: | GMT |
Daylight Saving Time: | OFF |
Name: |
Domain Name: |
WAN Interfaces
Interface | Encapsulation | IP Address | Mask | Gateway | Lower Interface | VPI/VCI | Status
ppp-0 | PPPoA | 85.70.119.111 | 255.255.255.255 | 80.188.61.122 | aal5-0 | 8/48 |
LAN Interface
Interface | Mac Address | IP Address | Mask | Lower Interface | Speed | Duplex | Status
eth-0 | 00:85:A0:01:01:00 | 10.0.0.138 | 255.255.255.0 | - | 100BT | Full |
usb-0 | - | 10.0.0.139 | 255.255.255.0 | - | - | - |
Services Summary
Interface | NAT | IP Filter | RIP | DHCP Relay | DHCP Client | DHCP Server | IGMP
eth-0 | inside |  |  |  |  |  |
ppp-0 | outside |  |  |  |  |  |
usb-0 | inside |  |  |  |  |  |