      < Mainboard and Processor(s) >
        Processor(s):                         Intel Pentium @ 198MHz
        Performance Rating:                   PR198  (estimated)
        System Bus(es):                       ISA(16-bit), PCI(32/64-bit)
        System BIOS:                          DMI Ver-2.0, Aug 24, 1995
        System Chipset:                       Intel Corporation 82437FX 430FX (Triton) Cache/DRAM
                                              Controller

      < System Memory >
        Installed Memory:                     64MB  (142% true allocated load)
        L2 External Cache:                    256kB pipeline-burst write-back

      < Video System >
        Monitor/Panel:                        Standaardmonitor
        Adapter:                              S3 Vision 968 PCI

      < Drives and Storage Devices >
        GENERIC IDE  DISK TYPE47:             C: 5.0GB
        GENERIC NEC  FLOPPY DISK:             A: 1.44MB 3.5"
        AZT 46801I          :                 D: (CD-ROM/DVD)

      < Peripherals >
        Serial/Parallel Port(s):              2 COM / 1 LPT
        Keyboard:                             Standaard- (101/102 toetsen) of Microsoft Natural-
                                              toetsenbord
        Mouse:                                Standaardmodel muis (serieel)

      < MultiMedia Device(s) >
        Device:                               Creative SB Live! Value
        Device:                               Creative gamepoort-joystick

      < Operating System(s) >
        Windows System:                       Microsoft Windows 98 Ver 4.10.2222  A
        DOS Sub-System:                       Microsoft MS-DOS Ver 7.10 A

      < Network Adapter(s) >
        Networking Installed:                 Yes
        Adapter:                              Externe-toegangsadapter
        Adapter:                              32-Bit PCI Fast Ethernet Adapter

    <<< Mainboard Information >>>
    -----------------------------------------------------------------------------------------------

      < General System Information >
        Class:                                IBM PC/AT
        System Bus(es):                       ISA(16-bit), PCI(32/64-bit)

      < System Chipset >
        System Chipset:                       Intel Corporation 82437FX 430FX (Triton) Cache/DRAM
                                              Controller
        L2 External Cache:                    256kB pipeline-burst write-back
        Front Side Bus Speed:                 66MHz

      < Logical/Chipset Memory Banks >
        Bank 1 Setting:                       32MB FPM 8-4-4-4R 6-3-3-3W
        Bank 3 Setting:                       32MB EDO 8-3-3-3R 6-3-3-3W
        Memory Bus Speed:                     66MHz

      < PCI Bus >
        Version:                              2.10
        Bus Speed:                            33MHz
        Speed Multiplier:                     1/2x

      < LPC/ISA Bus >
        PIIX Chip:                            Intel Corporation 82371FB PIIX PCI to ISA Bridge
        Speed Multiplier:                     1/4x
        Bus Speed:                            8MHz
        DMA Multiplier:                       1/2x
        DMA Speed:                            4MHz

      < Performance Tips >
        Notice N224:                          SMBIOS/DMI information may be inaccurate.
        Tip T2516:                            SDRAM, BEDO or EDO memory is recommended for optimum
                                              performance.
        Warning W2514:                        Memory read timing is high. Performance may be low.
        Tip T2:                               For more information about tips, press F1 and scroll
                                              to the Tips section.

    <<< CPU & BIOS Information >>>
    -----------------------------------------------------------------------------------------------

    << System BIOS >>
      < System BIOS >
        Manufacturer:                         American Megatrends
        Version:                              DMI Ver-2.0, Aug 24, 1995
        Date:                                 07/15/95
        Plug & Play Version:                  1.00
        ID No.:                               FC 01 00

      < Performance Tips >
        Tip T201:                             System BIOS is old. Check for an update.
        Tip T200:                             SMBIOS/DMI Interface not supported. Check for a BIOS
                                              update.
        Tip T2:                               For more information about tips, press F1 and scroll
                                              to the Tips section.

    << Processor 1 >>
      < Processor(s) >
        Processor:                            Intel Pentium @ 198MHz
        Co-Processor (FPU):                   Built-in
        Type:                                 Standard
        Performance Rating:                   PR198  (estimated)
        Class:                                5x86
        Model Information:                    P54C Pentium 75-233 3.3V
        Revision/Stepping:                    2 / C
        Stepping Mask:                        (m)cC0

      < Caches >
        Internal Code Cache:                  8kB synchronous write-back
        Internal Data Cache:                  8kB synchronous write-back

      < Features >
        Co-Processor (FPU) Built-in:          Yes
        Virtual Mode Extensions:              Yes
        Debugging Extension:                  Yes
        Page Size Extension:                  Yes
        Time Stamp Counter:                   Yes
        Model Specific Registers:             Yes
        Physical Address Extension:           No
        Machine Check Exception:              Yes
        Compare & Exchange Instruction:       Yes
        Local APIC Built-in:                  No
        Fast System Call:                     No
        Memory Type Range Registers:          No
        Page Global Enable:                   No
        Machine Check Architecture:           No
        Conditional Move Instruction:         No
        Page Attribute Table:                 No
        36-bit Page Size Extension:           No
        Unique Serial Number:                 No
        Cache Line Flush Support:             No
        Debug Trace & EMON Store:             No
        ACPI Support:                         No
        MMX Technology:                       No
        Fast Float Save & Restore:            No
        SSE Technology:                       No
        SSE2 Technology:                      No
        Self Snoop:                           No
        Auto Clock Control:                   No
        IA-64 Technology:                     No

      < Advanced Settings >
        Auto-Halt:                            Yes

      < Performance Tips >
        Tip T205:                             A MMX processor is recommended for modern multimedia
                                              applications and games.
        Tip T2:                               For more information about tips, press F1 and scroll
                                              to the Tips section.

    <<< APM & ACPI Information >>>
    -----------------------------------------------------------------------------------------------

      < APM BIOS >
        Version:                              1.01
        Program Support:                      16/32-bit
        System Status:                        Engaged
        AC Line Status:                       On-Line
        Battery Status:                       No System Battery

      < APM Capabilities >
        Supports Clock Slow-down:             No

      < APM System Status >
        AC Line Status:                       On-Line
        Battery Status:                       No System Battery

      < Performance Tips >
        Tip T1107:                            System does not support ACPI. Check for a BIOS
                                              update.
        Tip T1104:                            An APM BIOS Ver 1.02 or later may offer better
                                              performance/support. Check for a BIOS update.
        Warning W1101:                        Using APM on desktops may result in reduced
                                              performance or delays.
        Notice N224:                          SMBIOS/DMI information may be inaccurate.
        Tip T2:                               For more information about tips, press F1 and scroll
                                              to the Tips section.

    <<< PCI & AGP Buses Information >>>
    -----------------------------------------------------------------------------------------------

    << Buses Information >>
      < PCI & AGP Buses >
        Interface Version:                    2.10
        No. Buses:                            1
        Config space access mechanism 1 suppo:Yes
        Config space access mechanism 2 suppo:No
        Cycle generation mechanism 1 support: No
        Cycle generation mechanism 2 support: No

    << Intel Corporation 82437FX 430FX (Triton) Cache/DRAM Controller >>
      < Device Information >
        Device Type:                          Host Processor Bridge
        Device ID:                            Device 0h on bus 1 F0
        Windows Device Name:                  Intel 82437FX Pentium(r) Processor naar PCI-brug
        OEM Device Name:                      Intel Corporation 82437FX 430FX (Triton) Cache/DRAM
                                              Controller
        OEM Hardware ID:                      FUN_0, VEN_8086, DEV_122D
        Revision / Stepping:                  A / 2 (1)

      < Device Properties >
        Latency Timer:                        32 clocks
        I/O Access:                           No
        Memory Access:                        Yes
        Bus Master Capable:                   Yes
        Special Cycle Recognition:            No
        Memory Write & Invalidate:            No
        VGA Palette Snoop:                    No
        Parity Error Response:                No
        Address/Data Stepping:                No
        System Error Line:                    No
        Fast back-to-back Transactions:       No
        Detects Parity Errors:                No
        Supports System Error Line:           No
        Supports Parity Line:                 No
        User Defined Format:                  No
        PCI66 Bus Support:                    No
        New Capability List:                  No
        Device Select Timing:                 Medium
        Header Type:                          0

      < Hardware Resources >
        Dynamic Management:                   Yes

    << Intel Corporation 82371FB PIIX PCI to ISA Bridge >>
      < Device Information >
        Device Type:                          PCI to ISA Bridge
        Device ID:                            Device 7h on bus 1 F0
        Windows Device Name:                  Intel 82371FB PCI naar ISA-brug
        OEM Device Name:                      Intel Corporation 82371FB PIIX PCI to ISA Bridge
        OEM Hardware ID:                      FUN_0, VEN_8086, DEV_122E
        Revision / Stepping:                  A / 3 (2)

      < Device Properties >
        I/O Access:                           Yes
        Memory Access:                        Yes
        Bus Master Capable:                   Yes
        Special Cycle Recognition:            No
        Memory Write & Invalidate:            No
        VGA Palette Snoop:                    No
        Parity Error Response:                No
        Address/Data Stepping:                No
        System Error Line:                    No
        Fast back-to-back Transactions:       No
        Detects Parity Errors:                No
        Supports System Error Line:           No
        Supports Parity Line:                 No
        User Defined Format:                  No
        PCI66 Bus Support:                    No
        New Capability List:                  No
        Device Select Timing:                 Medium
        Header Type:                          0

      < Hardware Resources >
        Dynamic Management:                   Yes

    << Intel Corporation 82338/82371FB PIIX PCI EIDE Controller >>
      < Device Information >
        Device Type:                          EIDE Mass Storage Controller
        Device ID:                            Device 7h on bus 1 F1
        Windows Device Name:                  Intel 82371FB PCI Bus Master IDE-controller
        OEM Device Name:                      Intel Corporation 82338/82371FB PIIX PCI EIDE
                                              Controller
        OEM Hardware ID:                      FUN_1, VEN_8086, DEV_1230
        Revision / Stepping:                  A / 3 (2)

      < Device Properties >
        Latency Timer:                        32 clocks
        I/O Access:                           Yes
        Memory Access:                        No
        Bus Master Capable:                   Yes
        Special Cycle Recognition:            No
        Memory Write & Invalidate:            No
        VGA Palette Snoop:                    No
        Parity Error Response:                No
        Address/Data Stepping:                No
        System Error Line:                    No
        Fast back-to-back Transactions:       No
        Detects Parity Errors:                No
        Supports System Error Line:           No
        Supports Parity Line:                 No
        User Defined Format:                  No
        PCI66 Bus Support:                    No
        New Capability List:                  No
        Device Select Timing:                 Medium
        Header Type:                          0

      < Hardware Resources >
        I/O Port:                             FFA0
        I/O Port:                             01F0
        IRQ Line:                             14
        I/O Port:                             0170
        IRQ Line:                             15
        Dynamic Management:                   Yes

    << Creative Labs CT4850 SBLive! Value >>
      < Device Information >
        Device Type:                          Audio Multimedia Device
        Device ID:                            Device 11h on bus 1 F0
        Windows Device Name:                  Creative SB Live! Value
        OEM Device Name:                      Creative Labs EMU10K1 Audio Chipset
        OEM Hardware ID:                      FUN_0, VEN_1102, DEV_0002
        Product Device Name:                  Creative Labs CT4850 SBLive! Value
        Product Hardware ID:                  VEN_1102, DEV_0020
        Revision / Stepping:                  A / 5 (4)

      < Power Management Capabilities >
        Version:                              1.00
        Supports Clock Slow-down:             Yes
        Supports D1 PM State:                 No
        Supports D2 PM State:                 No
        Supports PME#:                        No
        Supports PME Clock:                   No

      < Device Properties >
        Latency Timer:                        64 clocks
        I/O Access:                           Yes
        Memory Access:                        No
        Bus Master Capable:                   Yes
        Special Cycle Recognition:            No
        Memory Write & Invalidate:            No
        VGA Palette Snoop:                    No
        Parity Error Response:                No
        Address/Data Stepping:                No
        System Error Line:                    Yes
        Fast back-to-back Transactions:       No
        Detects Parity Errors:                No
        Supports System Error Line:           No
        Supports Parity Line:                 No
        User Defined Format:                  No
        PCI66 Bus Support:                    No
        New Capability List:                  Yes
        Device Select Timing:                 Medium
        Header Type:                          0

      < Hardware Resources >
        I/O Port:                             EF80
        IRQ Line:                             9
        INT Pin:                              A#
        Dynamic Management:                   Yes

    << Creative Labs PCI Gameport Joystick >>
      < Device Information >
        Device Type:                          Other Input Device
        Device ID:                            Device 11h on bus 1 F1
        Windows Device Name:                  Creative MultiMedia-interface
        OEM Device Name:                      Creative Labs PCI Gameport Joystick
        OEM Hardware ID:                      FUN_1, VEN_1102, DEV_7002
        Product Device Name:                  Creative Labs PCI Gameport Joystick
        Product Hardware ID:                  VEN_1102, DEV_0020
        Revision / Stepping:                  A / 2 (1)

      < Power Management Capabilities >
        Version:                              1.00
        Supports Clock Slow-down:             Yes
        Supports D1 PM State:                 No
        Supports D2 PM State:                 No
        Supports PME#:                        No
        Supports PME Clock:                   No

      < Device Properties >
        Latency Timer:                        64 clocks
        I/O Access:                           Yes
        Memory Access:                        No
        Bus Master Capable:                   Yes
        Special Cycle Recognition:            No
        Memory Write & Invalidate:            No
        VGA Palette Snoop:                    No
        Parity Error Response:                No
        Address/Data Stepping:                No
        System Error Line:                    Yes
        Fast back-to-back Transactions:       No
        Detects Parity Errors:                No
        Supports System Error Line:           No
        Supports Parity Line:                 No
        User Defined Format:                  No
        PCI66 Bus Support:                    No
        New Capability List:                  Yes
        Device Select Timing:                 Medium
        Header Type:                          0

      < Hardware Resources >
        I/O Port:                             0200
        Dynamic Management:                   Yes

    << UNEX Technology Corp ND010 Fast Ethernet Adapter >>
      < Device Information >
        Device Type:                          Ethernet Network Adapter
        Device ID:                            Device 12h on bus 1 F0
        Windows Device Name:                  32-Bit PCI Fast Ethernet Adapter
        OEM Device Name:                      Realtek Semiconductor RT8139 (A/B/C/8130) Fast
                                              Ethernet Adapter
        OEM Hardware ID:                      FUN_0, VEN_10EC, DEV_8139
        Product Device Name:                  UNEX Technology Corp ND010 Fast Ethernet Adapter
        Product Hardware ID:                  VEN_1429, DEV_D010
        Revision / Stepping:                  B / 1 (16)

      < Power Management Capabilities >
        Version:                              2.00
        Supports Clock Slow-down:             Yes
        Supports D1 PM State:                 Yes
        Supports D2 PM State:                 Yes
        Supports PME#:                        Yes
        Supports PME Clock:                   No

      < Device Properties >
        Latency Timer:                        128 clocks
        I/O Access:                           Yes
        Memory Access:                        No
        Bus Master Capable:                   Yes
        Special Cycle Recognition:            No
        Memory Write & Invalidate:            No
        VGA Palette Snoop:                    No
        Parity Error Response:                No
        Address/Data Stepping:                No
        System Error Line:                    Yes
        Fast back-to-back Transactions:       No
        Detects Parity Errors:                No
        Supports System Error Line:           No
        Supports Parity Line:                 No
        User Defined Format:                  No
        PCI66 Bus Support:                    No
        New Capability List:                  Yes
        Device Select Timing:                 Medium
        Header Type:                          0

      < Hardware Resources >
        I/O Port:                             EC00
        Memory Address:                       FFAFFF00
        IRQ Line:                             10
        INT Pin:                              A#
        Dynamic Management:                   Yes

      < Performance Tips >
        Warning W1206:                        PCI latency too high. Device could hog the bus for
                                              too long.
        Tip T2:                               For more information about tips, press F1 and scroll
                                              to the Tips section.

    << S3 Inc 86C968 Vision 968 VRAM Rev 00 >>
      < Device Information >
        Device Type:                          VGA Display Adapter
        Device ID:                            Device 14h on bus 1 F0
        Windows Device Name:                  S3 Vision 968 PCI
        OEM Device Name:                      S3 Inc 86C968 Vision 968 VRAM Rev 00
        OEM Hardware ID:                      FUN_0, VEN_5333, DEV_88F0
        Revision / Stepping:                  A / 1 (0)

      < Device Properties >
        I/O Access:                           Yes
        Memory Access:                        Yes
        Bus Master Capable:                   No
        Special Cycle Recognition:            No
        Memory Write & Invalidate:            No
        VGA Palette Snoop:                    No
        Parity Error Response:                No
        Address/Data Stepping:                Yes
        System Error Line:                    No
        Fast back-to-back Transactions:       No
        Detects Parity Errors:                No
        Supports System Error Line:           No
        Supports Parity Line:                 No
        User Defined Format:                  No
        PCI66 Bus Support:                    No
        New Capability List:                  No
        Device Select Timing:                 Medium
        Header Type:                          0

      < Hardware Resources >
        Memory Address:                       80000000
        IRQ Line:                             11
        INT Pin:                              A#
        Expansion ROM:                        7F000000
        Dynamic Management:                   Yes

      < Performance Tips >
        Warning W1201:                        Early versions of hardware may contain bugs or
                                              incompatibilities.
        Tip T1202:                            Device does not support bus mastering.
        Tip T2:                               For more information about tips, press F1 and scroll
                                              to the Tips section.

    -----------------------------------------------------------------------------------------------
    *****  End of Report - Report created successfully  *****