servlinux

description: | Computer
product: | PRIMERGY ECONEL 50
vendor: | FUJITSU SIEMENS
version: | EC50F
serial: | S26361-K831-V51
capabilities: | smbios-2.31 dmi-2.31

core

description: | Motherboard
product: | D1859
vendor: | FUJITSU SIEMENS
physical id: | 0
version: | S26361-D1859
serial: | B0253E10
slot: | Serial-1

firmware

description: | BIOS
vendor: | FUJITSU SIEMENS // Phoenix Technologies Ltd.
physical id: | 0
version: | 4.06 Rev. 1.03.1859 (06/21/2005)
size: | 107KB
capacity: | 448KB
capabilities: | pci pnp apm upgrade shadowing escd cdboot bootselect int13floppynec int13floppytoshiba int13floppy360 int13floppy1200 int13floppy720 int13floppy2880 int5printscreen int9keyboard int14serial int17printer int10video acpi usb ls120boot zipboot biosbootspecification

cpu UNCLAIMED

description: | CPU
vendor: | Intel
physical id: | 4
version: | Intel(R) Pentium(R) 4 CPU
slot: | CPU
size: | 3GHz
capacity: | 3GHz
clock: | 800MHz

cache:0 UNCLAIMED

description: | L1 cache
physical id: | 5
slot: | L1 Cache
size: | 16KB
capacity: | 32KB
capabilities: | burst synchronous internal write-through data

cache:1 UNCLAIMED

description: | L2 cache
physical id: | 6
slot: | L2 Cache
size: | 1MB
capacity: | 1MB
capabilities: | burst internal write-back

cache:2 DISABLED UNCLAIMED

description: | L3 cache
physical id: | 7
slot: | L3 Cache
capacity: | 16MB
capabilities: | internal write-back

memory

description: | System Memory
physical id: | 26
slot: | System board or motherboard
size: | 512MB

bank:0

description: | DIMM Synchronous 533 MHz (1.9 ns)
physical id: | 0
slot: | Slot-1
size: | 512MB
clock: | 533MHz (1.87617ns)
configuration: |
width | = | 72/64

bank:1

description: | DIMM Synchronous 533 MHz (1.9 ns)
physical id: | 1
slot: | Slot-3
clock: | 533MHz (1.87617ns)

bank:2

description: | DIMM Synchronous 533 MHz (1.9 ns)
physical id: | 2
slot: | Slot-2
clock: | 533MHz (1.87617ns)

bank:3

description: | DIMM Synchronous 533 MHz (1.9 ns)
physical id: | 3
slot: | Slot-4
clock: | 533MHz (1.87617ns)

pci

physical id: | 100
bus info: | pci@00:00.0
version: | 04
clock: | 33MHz

display UNCLAIMED

physical id: | 2
bus info: | pci@00:02.0
version: | 04
size: | 256MB
clock: | 33MHz
capabilities: | bus_master cap_list
resources: |
iomemory | : | f0000000-f007ffff
ioport | : | 1000-1007
iomemory | : | e0000000-efffffff
iomemory | : | f0080000-f00bffff
irq | : | 16

pci:0

physical id: | 1c
bus info: | pci@00:1c.0
version: | 03
clock: | 33MHz
capabilities: | pci cap_list

pci:1

physical id: | 1c.1
bus info: | pci@00:1c.1
version: | 03
clock: | 33MHz
capabilities: | pci cap_list

pci:2

physical id: | 1c.2
bus info: | pci@00:1c.2
version: | 03
clock: | 33MHz
capabilities: | pci bus_master cap_list

network UNCLAIMED

physical id: | 0
bus info: | pci@07:00.0
version: | 11
clock: | 33MHz
capabilities: | bus_master cap_list
resources: |
iomemory | : | f0100000-f010ffff
irq | : | 18

pci:3

physical id: | 1c.3
bus info: | pci@00:1c.3
version: | 03
clock: | 33MHz
capabilities: | pci cap_list

usb:0

physical id: | 1d
bus info: | pci@00:1d.0
version: | 03
clock: | 33MHz
capabilities: | bus_master
configuration: |
driver | = | uhci_hcd
resources: |
ioport | : | 2400-241f
irq | : | 23

usb:1

physical id: | 1d.1
bus info: | pci@00:1d.1
version: | 03
clock: | 33MHz
capabilities: | bus_master
configuration: |
driver | = | uhci_hcd
resources: |
ioport | : | 2800-281f
irq | : | 22

usb:2

physical id: | 1d.2
bus info: | pci@00:1d.2
version: | 03
clock: | 33MHz
capabilities: | bus_master
configuration: |
driver | = | uhci_hcd
resources: |
ioport | : | 2c00-2c1f
irq | : | 21

usb:3

physical id: | 1d.3
bus info: | pci@00:1d.3
version: | 03
clock: | 33MHz
capabilities: | bus_master
configuration: |
driver | = | uhci_hcd
resources: |
ioport | : | 3000-301f
irq | : | 20

usb:4

physical id: | 1d.7
bus info: | pci@00:1d.7
version: | 03
clock: | 33MHz
capabilities: | bus_master cap_list
configuration: |
driver | = | ehci_hcd
resources: |
iomemory | : | f00c0000-f00c03ff
irq | : | 23

pci:4

physical id: | 1e
bus info: | pci@00:1e.0
version: | d3
clock: | 33MHz
capabilities: | pci bus_master cap_list

network UNCLAIMED

physical id: | 5
bus info: | pci@0b:05.0
version: | 10
clock: | 33MHz
capabilities: | bus_master
resources: |
ioport | : | 4000-40ff
iomemory | : | f0200000-f02000ff
irq | : | 22

isa UNCLAIMED

physical id: | 1f
bus info: | pci@00:1f.0
version: | 03
clock: | 33MHz
capabilities: | isa bus_master

ide

physical id: | 1f.2
bus info: | pci@00:1f.2
version: | 03
clock: | 66MHz
capabilities: | ide bus_master cap_list
configuration: |
driver | = | ata_piix
resources: |
ioport | : | 3800-380f
irq | : | 19

serial UNCLAIMED

physical id: | 1f.3
bus info: | pci@00:1f.3
version: | 03
clock: | 33MHz
resources: |
ioport | : | 3400-341f
irq | : | 19

scsi

physical id: | 1
bus info: | scsi@2
logical name: | scsi2
configuration: |
driver | = | usb-storage

network DISABLED

description: | controller
physical id: | 2
logical name: | sit0