1. Dmesg output attached.

2. Kernel is :kernel-PAE.i686 3.11.6

3. Display resolution is 1920x1200

4. Video card : IBM Intellistation Graphics Card FRU IBM 25P6684 NVIDIA Quadro4 200NVS 64MB

5. xorg-x11-drv-nouveau.i686 1:1.0.9-1.fc19

6. mesa-dri-drivers.i686 9.2-1.20130919.fc19
mesa-filesystem.i686 9.2-1.20130919.fc19
mesa-libEGL.i686 9.2-1.20130919.fc19
mesa-libGL.i686 9.2-1.20130919.fc19
mesa-libGLU.i686 9.0.0-2.fc19
mesa-libgbm.i686 9.2-1.20130919.fc19
mesa-libglapi.i686 9.2-1.20130919.fc19
mesa-libwayland-egl.i686 9.2-1.20130919.fc19
mesa-libxatracker.i686 9.2-1.20130919.fc19

7. OS is Linux Fedora 19

8. System has 4GB memory.

From: bugzilla-daemon@freedesktop.org <bugzilla-daemon@freedesktop.org>
Sent: November-09-13 17:40
To: Brian Kaye
Subject: [Bug 71438] [NV10/nouveau_vieux] Application Konqueror crashes when connecting to asus.com
Ilia Mirkin changed bug 71438

What | Removed | Added
--- | --- | ---
Summary | Application Konqueror crashes when connecting to asus.com | [NV10/nouveau_vieux] Application Konqueror crashes when connecting to asus.com

Comment # 1 on bug 71438 from Ilia Mirkin

    The relevant bit of the stacktrace:

    #10 0x42834a87 in __assert_fail () from /lib/libc.so.6
    #11 0xaf348070 in nouveau_scratch_init () from
    /usr/lib/dri/nouveau_vieux_dri.so
    #12 0xaf3436ed in nouveau_context_init () from
    /usr/lib/dri/nouveau_vieux_dri.so
    #13 0xaf34d811 in nv10_context_create () from /usr/lib/dri/nouveau_vieux_dri.so
    #14 0xaf343abd in nouveau_context_create () from
    /usr/lib/dri/nouveau_vieux_dri.so
    #15 0xaf36045f in dri2CreateContextAttribs () from
    /usr/lib/dri/nouveau_vieux_dri.so
    #16 0xaf360638 in dri2CreateNewContext () from
    /usr/lib/dri/nouveau_vieux_dri.so
    #17 0xb4032024 in dri2_create_context () from /lib/libGL.so.1
    #18 0xb400824a in CreateContext () from /lib/libGL.so.1
    #19 0xb4008541 in glXCreateContext () from /lib/libGL.so.1

    And the code in nouveau_scratch_init:

        for (i = 0; i < NOUVEAU_SCRATCH_COUNT; i++) {
            ret = nouveau_bo_new(context_dev(ctx), NOUVEAU_BO_GART |
                         NOUVEAU_BO_MAP, 0, NOUVEAU_SCRATCH_SIZE,
                         NULL, &scratch->bo[i]);
            assert(!ret);

    Looks like it's trying to get 2 3MB bo's, but it can't. Unfortunately error
    handling is often done rather poorly in the nouveau_vieux driver (via asserts
    rather than returning error codes).

    What card are you using? How much VRAM does it have? What resolution are you
    running your screen at? What kernel are you on? What version of
    xf86-video-nouveau and mesa are you using?

You are receiving this mail because:

- You reported the bug.